Alexis Fuerte  
CS – 350  
10 July 2022  
 Module 2  
• What does pwmled2 set the PWM period to?   
3000 Microseconds  
• Which PWM\_xxx() function sets the PWM period?   
PWM\_Params\_init  
• Which PWM\_xxx() function sets the PWM duty cycle?   
PWM\_setDuty  
• What is the purpose of the while(1) loop in pwmled2?   
The while loop keeps the function running forever (or until told to stop), so the yellow and green lights will continue to blink  
• What is the purpose of usleep() in the while(1) loop?   
Usleep gives the lights some time in between blinking, in this case it gives 1 second in between blinks