Alexis Fuerte  
CS-350  
31 July 2022  
 Milestone 3  
What is the purpose of the timerCallback() function?

Performs the actions of the state machine after a specific time period

What does period mean in this context?

The amount of time that one tick takes is a period.

How does the Timer\_CONTINUOUS\_CALLBACK parameter impact the driver?

The timerCallback() function is called after each interrupt and the user routine is not blocked.

What is gpioButtonFxn0() used for?

It is used to set the state to SOS.

What is the purpose of GPIO\_CFG\_IN\_INT\_FALLING?

It’s a configuration for button 0.